NYX-512 ECoG Probe Reference Design (KiCad)
Science Corporation
05/2026
v1.0

Contents
--------
NYX1-512 ECoG Probe.kicad_pro   KiCad project file
NYX1-512 ECoG Probe.kicad_pcb   PCB layout
NYX1-512 ECoG Probe.kicad_sch   Top-level schematic (title/cover page)
NYX1_512_ECoG.kicad_sch          Circuit sub-sheet

Requirements
------------
KiCad 10 or later.

The NYX512 KiCad component library (NYX512-KiCad-Library.zip)
must be installed before opening this project. See that package's
README for setup instructions.

Setup
-----
1. Install the NYX512 KiCad component library first.
2. Open NYX1-512 ECoG Probe.kicad_pro in KiCad.

Notes
-----
- This is a complete routing reference for the NYX-512 recording 
  ASIC. This example shows NYX-512 routing for a polyimide thin film 
  ECoG neural probe.
- The design has two schematic sheets. The top-level sheet is a
  cover/title page. The sub-sheet (NYX1_512_ECoG) contains the
  actual circuit.
- If KiCad reports missing symbols or footprints, verify the
  NYX512 libraries are registered under Preferences -> Manage
  Symbol/Footprint Libraries.
